{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":27,"n_cols":12,"rows_kept":27,"merged":[[0,0,0,11],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,5,1,10],[3,1,6,1],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,12,1],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,21,1],[22,1,25,1],[26,1,26,11]]}
["空压机常规维修清单"]
["序号","维修项目","维修内容","单位","数量","含13%增值税单价/元",{"$nulls":5},"备注"]
[{"$nulls":5},"优耐特斯 UDT160A-8VPM","优耐特斯UD55A-8C","阿特拉斯 GA-75","意朗 ERC-75SA","意朗 ERC-100SA","宝勒特BLT25A-3/8"]
[1,"主机电机维修","绕线圈（包括修线圈、更换轴承、油封、修复轴头在内）","个",1]
[2,null,"漏油（包括更换油封、轴承）","个",1]
[3,null,"整台电机更换新机","个",1]
[4,null,"阿特拉斯机型主电机后端轴承维修更换","个",1]
[5,"加载阀维修更换",null,"个",1]
[6,"温控阀维修更换",null,"个",1]
[7,"温度传感器维修更换",null,"个",1]
[8,"压力传感器维修更换",null,"个",1]
[9,"控制屏","维修","个",1]
[10,null,"更换新屏","个",1]
[11,"水冷散热器油管维修更换",null,"个",1]
[12,"进气管维修更换",null,"个",1]
[13,"进气阀维修更换",null,"个",1]
[14,"回油管维修更换",null,"个",1]
[15,"主机电机电动散热风扇",null,"个",1]
[16,"主机散热器维修更换",null,"个",1]
[17,"主机散热器散热风机维修","更换叶轮","个",1]
[18,null,"更换电机","个",1]
[19,null,"维修电机线圈及更换轴承","个",1]
[20,"主机机头维修","维修更换轴承","个",1]
[21,null,"维修更换密封","个",1]
[22,null,"螺杆轴头修复","个",1]
[23,null,"机头整机更换维修","个",1]
[24,"以上维修质保期一年。明细以外维修另定（常规接触器、继电器、开关、PLC模块、热继电器、按钮、钮子开关等电气原件由华昌负责购买）。"]