{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":63,"n_cols":9,"rows_kept":63,"merged":[[0,0,0,8],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,4],[1,5,1,7],[1,8,2,8],[3,3,3,4],[4,3,4,4],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,5,4],[6,3,6,4],[7,0,8,0],[7,1,8,1],[7,2,8,2],[7,3,7,4],[8,3,8,4],[9,0,10,0],[9,1,10,1],[9,2,10,2],[9,3,9,4],[10,3,10,4],[11,0,12,0],[11,1,12,1],[11,2,12,2],[11,3,11,4],[12,3,12,4],[13,0,14,0],[13,1,14,1],[13,2,14,2],[13,3,13,4],[14,3,14,4],[15,3,15,4],[16,3,16,4],[17,3,17,4],[18,3,18,4],[19,3,19,4],[20,3,20,4],[21,3,21,4],[22,3,22,4],[23,3,23,4],[24,0,25,0],[24,1,25,1],[24,2,25,2],[24,3,24,4],[25,3,25,4],[26,0,27,0],[26,1,27,1],[26,2,27,2],[26,3,26,4],[27,3,27,4],[28,0,29,0],[28,1,29,1],[28,2,29,2],[28,3,28,4],[29,3,29,4],[30,0,31,0],[30,1,31,1],[30,2,31,2],[30,3,30,4],[31,3,31,4],[32,0,33,0],[32,1,33,1],[32,2,33,2],[32,3,32,4],[33,3,33,4],[34,0,35,0],[34,1,35,1],[34,2,35,2],[34,3,34,4],[35,3,35,4],[36,0,37,0],[36,1,37,1],[36,2,37,2],[36,3,36,4],[37,3,37,4],[38,0,39,0],[38,1,39,1],[38,2,39,2],[38,3,38,4],[39,3,39,4],[40,0,41,0],[40,1,41,1],[40,2,41,2],[40,3,40,4],[41,3,41,4],[42,3,42,4],[43,3,43,4],[44,3,44,4],[45,3,45,4],[46,3,46,4],[47,3,47,4],[48,3,48,4],[49,3,49,4],[50,0,51,0],[50,1,51,1],[50,3,51,4],[50,5,51,5],[50,6,51,6],[50,7,51,7],[50,8,51,8],[52,0,53,0],[52,1,53,1],[52,3,53,4],[52,5,53,5],[52,6,53,6],[52,7,53,7],[52,8,53,8],[54,0,55,0],[54,1,55,1],[54,3,55,4],[54,5,55,5],[54,6,55,6],[54,7,55,7],[54,8,55,8],[56,0,57,0],[56,1,57,1],[56,3,57,4],[56,5,57,5],[56,6,57,6],[56,7,57,7],[56,8,57,8],[58,3,58,4],[59,3,59,4],[60,3,60,4],[61,3,61,4],[62,2,62,7]],"flags":["formulas_cached_only"]}
["2024年环境监测项目"]
["序号","项目类别","检测点位","检测项目",null,"检测频次",null,null,"备注"]
[{"$nulls":5},"点数","次/年","天数"]
[1,"有组织熔铸废气FQ-21951-1","处理后1个监测口","林格曼黑度",null,1,"1次/年",1,"2024年监测1次"]
[2,"有组织熔铸废气FQ-21951-2","处理后1个监测口","林格曼黑度",null,1,"1次/年",1,"2024年监测1次"]
[3,"有组织搓灰废气FQ-21951-3","处理后1个监测口","颗粒物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[{"$nulls":3},"氟及其化合物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[4,"有组织电泳固化废气FQ-21951-4","处理后1个监测口","颗粒物、二氧化硫、氮氧化物、总VOCs",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/年",1,"2024年监测1次"]
[5,"有组织电泳固化废气FQ-21951-5","处理后1个监测口","颗粒物、二氧化硫、氮氧化物、总VOCs",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/年",1,"2024年监测1次"]
[6,"有组织电泳固化废气FQ-21951-6","处理后1个监测口","颗粒物、二氧化硫、氮氧化物、总VOCs",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/年",1,"2024年监测1次"]
[7,"有组织喷涂废气FQ-21951-7","处理后1个监测口","苯、甲苯+二甲苯",null,1,"1次/季",4,"2024年第一季度到第四季度，共监测4次"]
[{"$nulls":3},"总VOCs",null,1,"1次/月",12,"2024年1月到12月，共监测12次"]
[8,"有组织前处理废气FQ-21951-8","处理后1个监测口","硫酸雾、氮氧化物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[9,"有组织前处理废气FQ-21951-9","处理后1个监测口","碱雾",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[10,"有组织前处理废气FQ-21951-10","处理后1个监测口","硫酸雾、氮氧化物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[11,"有组织前处理废气FQ-21951-11","处理后1个监测口","碱雾",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[12,"有组织前处理废气FQ-21951-12","处理后1个监测口","硫酸雾、氮氧化物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[13,"有组织前处理废气FQ-21951-13","处理后1个监测口","碱雾",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[14,"有组织煲模废气FQ-21951-14","处理后1个监测口","碱雾",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[15,"有组织喷粉废气FQ-21951-15","处理后1个监测口","颗粒物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[16,"有组织喷粉废气FQ-21951-16","处理后1个监测口","颗粒物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[17,"有组织棒炉废气FQ-21951-17","处理后1个监测口","颗粒物、二氧化硫、氮氧化物",null,1,"1次/月",12,"2024年1月到12月，共监测12次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[18,"有组织棒炉废气FQ-21951-18","处理后1个监测口","颗粒物、二氧化硫、氮氧化物",null,1,"1次/月",12,"2024年1月到12月，共监测12次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[19,"有组织棒炉废气FQ-21951-19","处理后1个监测口","颗粒物、二氧化硫、氮氧化物",null,1,"1次/月",12,"2024年1月到12月，共监测12次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[20,"有组织棒炉废气FQ-21951-20","处理后1个监测口","颗粒物、二氧化硫、氮氧化物",null,1,"1次/月",12,"2024年1月到12月，共监测12次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[21,"有组织棒炉废气FQ-21951-21","处理后1个监测口","颗粒物、二氧化硫、氮氧化物",null,1,"1次/月",12,"2024年1月到12月，共监测12次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[22,"有组织棒炉废气FQ-21951-22","处理后1个监测口","颗粒物、二氧化硫、氮氧化物",null,1,"1次/月",12,"2024年1月到12月，共监测12次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[23,"有组织时效废气FQ-21951-23","处理后1个监测口","颗粒物、二氧化硫、氮氧化物",null,1,"1次/月",12,"2024年1月到12月，共监测12次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[24,"有组织时效废气FQ-21951-24","处理后1个监测口","颗粒物、二氧化硫、氮氧化物",null,1,"1次/月",12,"2024年1月到12月，共监测12次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[25,"有组织均质废气FQ-21951-25","处理后1个监测口","颗粒物、二氧化硫、氮氧化物",null,1,"1次/月",12,"2024年1月到12月，共监测12次"]
[{"$nulls":3},"林格曼黑度",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[26,"有组织喷砂废气FQ-21951-26","处理后1个监测口","颗粒物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[27,"有组织喷砂废气FQ-21951-27","处理后1个监测口","颗粒物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[28,"有组织喷砂废气FQ-21951-28","处理后1个监测口","颗粒物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[29,"有组织喷砂废气FQ-21951-29","处理后1个监测口","颗粒物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[30,"有组织喷砂废气FQ-21951-30","处理后1个监测口","颗粒物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[31,"有组织喷粉废气FQ-21951-31","处理后1个监测口","颗粒物",null,1,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[32,"车间预处理口","预处理后1个监测口","总镍",null,1,"1次/日（按月手工测）",12,"2024年1月到12月，共监测12次"]
[33,"综合废水处理(WS-21951-1)","处理后1个监测口","SS、CODCr、氨氮、总氮、总磷、石油类、氟化物、总铝",null,1,"1次/月",12,"2024年1月到12月，共监测12次"]
[34,"厂界无组织废气","上风向1个点，","苯、甲苯、二甲苯、总VOCs",null,4,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[null,null,"下风向3个点"]
[35,"厂界无组织废气","上风向1个点，","氮氧化物",null,4,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[null,null,"下风向3个点"]
[36,"厂界无组织废气","上风向1个点，","硫酸雾",null,4,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[null,null,"下风向3个点"]
[37,"厂界无组织废气","上风向1个点，","颗粒物",null,4,"1次/半年",2,"2024年上半年监测1次，下半年监测1次，共2次"]
[null,null,"下风向3个点"]
[38,"车间无组织废气","初拟门口设置1个点","非甲烷总烃",null,1,"1次/年",1,"2024年监测1次"]
[39,"噪声","4个点","厂界噪声（昼间）",null,1,"1次/季",4,"2024年第一季度到第四季度，共监测4次"]
[41,"有组织熔铸废气FQ-21951-1","1台在线监控","颗粒物、二氧化硫、氮氧化物、含氧量、烟气流速、烟气温度、烟气湿度",null,1,"1次/季",4,"2024年第一季度到第四季度，共监测4次"]
[42,"有组织熔铸废气FQ-21951-2","1台在线监控","颗粒物、二氧化硫、氮氧化物、含氧量、烟气流速、烟气温度、烟气湿度",null,1,"1次/季",4,"2024年第一季度到第四季度，共监测4次"]
[43,"国家排污证平台管理手续","1、国家排污平台日常维护\n2、信息填报\n3、网上提交信息环保办\n4、执行报告填报和上传\n5、协助台账登记（主要信息需要企业根据实际提供或者填报）\n6、自行监测信息填报",{"$nulls":5},"2024第一季度至2024第四季度（12个月）"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}